# File generated by Wizard 2.9.0 on Feb 3, 2026.
platform_type YY20 WSF_PLATFORM 
   icon tanker
   side red
   infrared_signature VEHICLE_INFRARED_SIGNATURE
   optical_signature VEHICLE_OPTICAL_SIGNATURE
   radar_signature VEHICLE_RADAR_SIGNATURE

   mover   WSF_AIR_MOVER   
      update_interval 1 seconds    
      maximum_impact_speed 300 m/s    
      altitude_offset 20 meters    
      at_end_of_path stop        
      turn_failure_threshold 0.01        
      bank_angle_limit 5 degrees    
      heading_pursuit_gain 5        
      maximum_flight_path_angle 70 degrees    
      maximum_linear_acceleration 6 g    
      maximum_radial_acceleration 6 g    
      maximum_altitude 50000 ft 
      minimum_altitude 50 ft    
      maximum_speed 450 m/s    
      minimum_speed 300 m/s    
      speed_variance_percent 0.0        
      roll_rate_limit 1 rad/sec    
      maximum_climb_rate 365 m/s    
      default_linear_acceleration 1 g    
      default_radial_acceleration 6.5 g    
      default_climb_rate 122 m/s      
   end_mover
   
   sensor eo_ir_sensor common_geo_radar
      on
      internal_link track_manager
      internal_link data_mgr
      ignore_same_side
   end_sensor
   
   comm sub_net TEAM_DATALINK
      network_name red_net
      internal_link track_manager
      internal_link data_mgr
   end_comm
   processor track_manager WSF_TRACK_PROCESSOR
      purge_interval 60 sec
      report_interval 5 sec
      report_method batch
      report_to commander via sub_net
   end_processor
   fuel   WSF_VARIABLE_RATE_FUEL   
      rate   0.5 kg/s    
      maximum_quantity 99999 kg    
      initial_quantity 99999 kg 
      bingo_quantity 2000 kg     
   end_fuel  
    
   processor data_mgr WSF_TRACK_PROCESSOR
      purge_interval 60 sec
      update_interval 1 sec
   end_processor   
end_platform_type