# File generated by Wizard 2.9.0 on Feb 8, 2026.
# File generated by Wizard 2.9.0 on Jan 25, 2026.
# File generated by Wizard 2.9.0 on Dec 23, 2024.
# File generated by Wizard 2.9.0 on Jun 6, 2024.
# --------------------------------------------------------------
#                         Vehicle Signatures
# --------------------------------------------------------------
include_once sensors/radar/acq_radar.txt
infrared_signature  VEHICLE_INFRARED_SIGNATURE
   constant  10 watts/steradian
end_infrared_signature

optical_signature   VEHICLE_OPTICAL_SIGNATURE
   constant  10 m^2
end_optical_signature

radar_signature     VEHICLE_RADAR_SIGNATURE
   constant  1 m^2
end_radar_signature

# --------------------------------------------------------------
#                         Red datalink
# --------------------------------------------------------------

comm TEAM_DATALINK WSF_COMM_TRANSCEIVER
   transfer_rate      100 mbits/sec
end_comm
#   
comm CC_DATALINK WSF_RADIO_TRANSCEIVER
   transmitter 
      antenna_pattern          ACQ_RADAR_ANTENNA
      power                    1000.0 kw
      frequency                3000 mhz
      internal_loss            2 db
      bandwidth                237 mhz
   end_transmitter
   
   receiver
      antenna_pattern          ACQ_RADAR_ANTENNA
      bandwidth                2.0 mhz
      noise_power              -160 dbw // will be calibrated for 1 m^2
      internal_loss            7 db
      bandwidth                237 mhz
   end_receiver
end_comm

network red_net WSF_COMM_NETWORK_MESH 
end_network

# --------------------------------------------------------------
#                         Filter tactics
# --------------------------------------------------------------

filter FILTER_TACTICS WSF_KALMAN_FILTER
   range_measurement_sigma       50. m
   bearing_measurement_sigma     0.1 deg
   elevation_measurement_sigma   0.1 deg

   // values for maneuvering targets (per Erik)
   process_noise_sigmas_XYZ  50 50 30
end_filter



//
//the new DATALINK
//
antenna_pattern DATALINK_ANTENNA
   uniform_pattern
      peak_gain 10 dB
   end_uniform_pattern
end_antenna_pattern
comm DATALINK WSF_RADIO_TRANSCEIVER
   maximum_range 50 km
   transfer_rate 100 mbits/sec
   transmit_mode continuous
   
   transmitter
      power 100 w
      frequency 1.5 GHz //the matter
      bandwidth 10 MHz
      antenna_pattern DATALINK_ANTENNA
   end_transmitter
   
   receiver
      frequency 1.5 GHz
      bandwidth 10 MHz
      antenna_pattern DATALINK_ANTENNA
   end_receiver
   
   jamming_perception_threshold 3 db  
   jamming_perception_timeout 60 sec
end_comm

